**TYT UV380 Basic Operation Suggestions**

**Select = Green button**

**Go back = Red button**

**-Select a Zone:**

Select🡪up/down arrow highlight zone🡪select🡪zone list🡪select🡪up/down to zone name🡪select

Use up and down side buttons to change zones

**-Select a channel for that zone:**

Turn knob in middle to desired channel

**-Turn scanning on/off for a zone (not available for Hot Spot)**

select🡪up/down arrow highlight scan🡪select🡪on🡪select

Long press on top left side button

To turn off, turn the middle know on the radio one click or long press on top left side button

**-Operating tips**

ARRL recommends as a good practice you listen first, except for a Hot Spot

Hot Spots are a PTT device, meaning you must key up the talk group want and then listen

Suggest you leave space while talking between transmissions.

Understand that sometimes transmission may be interrupted or not go through. Try again

Listen on [http://hose.brandmeister.network/group/#####/](http://hose.brandmeister.network/group/#/) where ##### is the Talk Group Number